* + 1. Digital Keypad, Integrated, Indoor /Outdoor:

Product: Model 920 Indoor/Outdoor EntryCheck as manufactured by SDC. Single gang keypad with 500 users. User Codes to be 4 to 6 digits in length, programmable for individual or simultaneous control of 2 relay outputs momentary, timed or latching with 2 additional programmable solid state outputs

* + - * 1. Two LEDs - Output Red/Green and Amber status indicators.
        2. Four Outputs: Relay #1, SPDT, 5 Amps at 30 V. Relay #2, SPDT, 2 Amp at 30 V. Output #3 and #4, solid state open collectors 100 mA at 24 VDC.
        3. Voltage: 12/24 VDC or AC (AC supply shall be transformer isolated).

Current: 30 mA typical, 150 mA maximum.

* + - * 1. Automatic time-out REX input,
        2. Choice of function for Sense input - Keypad disable or Door Sense

1. Forced Entry
2. Door ajar
3. Inhibit Relay 1 or 2
4. Auto relock when door closes
   * + - 1. Choice of function for Relay #2 and two solid state outputs #3 & #4
5. Alarm shunt
6. Forced entry
7. Door ajar
8. Tamper lockout
9. Keypad active
   * + - 1. Timed Anti-tailgate
         2. Blue illuminated keys with tactile feel
         3. Single gang rugged cast housing (5.75”Hx 3.00”Wx 1.375”D)
         4. Operating Temperature; -4 degree F to +140 degree F (-20 degree C to +60 degree C).
         5. Humidity: 5% to 95%, non-condensing.