* 1. STAND ALONE LOCKSETS
     1. Battery Powered Mortise Lockset with Digital Keypad and HID Compatible Prox Card/FOB Reader
        1. Product: Model **E76P** - EntryCheck Standalone Mortise Lockset with Digital Keypad and HID compatible Prox Card/FOB Reader as manufactured by SDC Security Door Controls.
           1. Battery powered electronic mortise lockset for 3000 users. Standard features include an ANSI Grade 1 Mortise lockset with a lever clutch mechanism, 4-6 digit pin code, all weather keypad and housing, keypad or computer programming, 32 user groups, multi-year scheduling, temporary users, multiple zones, real time clock, auto daylight savings adjustment and more.
           2. Mortise lockset with 3/4 inch (19 mm) latch bolt with deadlatch. 4-7/8 inch (124 mm) strike standard.
           3. HID compatible Proximity card and/or Proximity FOB reader
           4. UL Listed, USA and Canada for 3 hour "A" label fire rated doors. ANSI A156.25, Electrified Lockset Compliant. ANSI A156.13 Grade 1 Compliant.
           5. ANSI A117.1 Accessibility Code Compliant. ADA Compliant. California State Reference Code (Formerly Title 19, California State Fire Marshal): Compliant. Levers Galaxy, Eclipse and Nova return to within 1/2 inch (13mm) of the door face.

\*\* NOTE TO SPECIFIER \*\* Lever Handles with/without cylinders. Delete lever not required.

* + - 1. Handing: L - Left hand.
      2. Handing: LR - Left hand reverse
      3. Handing: R - Right hand.
      4. Handing: RR - Right hand reverse

\*\* NOTE TO SPECIFIER \*\* Black Dull Chrome is standard. Delete finish for keypad and lock that are not required.

* + - 1. Lever Trim: G - Galaxy with rose.
      2. Lever Trim: GE - Galaxy with escutcheon.
      3. Lever Trim: E - Eclipse with rose.
      4. Lever Trim: EE - Eclipse with escutcheon.
      5. Lever Trim: N - Nova with rose.
      6. Lever Trim: NE - Nova with escutcheon.
      7. Lever Trim: 07 - Schlage equivalent with SDC B rose.
      8. Lever Trim: 07E - Schlage equivalent with SDC escutcheon.
      9. Keypad Finish:

Q - Dull chrome

B – Black

* + - 1. Lock and Trim Finish:
         1. Q- Dull chrome
         2. C – Polished Brass
         3. P – Bright Chrome
      2. Keyed Cylinder Optional: CYL-6KDQ - 6 pin, 1.125 inches (29 mm) mortise cylinder, keyed different, dull chrome.
      3. Keyed Cylinder Optional: CYL-6KAQ - 6 pin, 1.125 inches (29 mm) mortise cylinder, keyed alike, dull chrome.
      4. Optional - Card: HID1326-100 ProxCard II (100 cards) as manufactured by SDC Security Door Controls.
      5. Optional - Card: HID1326-25 ProxCard II (25 cards) as manufactured by SDC Security Door Controls.
      6. Optional - Key Fob: HID1346-10 ProxKey II (10 key fobs) as manufactured by SDC Security Door Controls.
      7. Optional - Key Fob: HID1346-100 ProxKey II (100 key fobs) as manufactured by SDC Security Door Controls.