* 1. STANDALONE RIM EXIT BAR
     1. SDC S6100 Rim Exit bar with battery powered electrically operated Escutcheon Trim, Digital Keypad and HID Compatible Proximity Reader
        1. Product: Model **E77P** - EntryCheck Standalone Rim Exit Bar with Electrically operated Escutcheon Trim, Digital Keypad and HID compatible Prox Card/FOB Reader as manufactured by SDC Security Door Controls.
           1. Battery powered electronic keypad and HID compatible Prox reader for 3000 users. Standard features include an ANSI Grade 1 SDC S6100 Rim Exit bar with electrically operated escutcheon lever trim, 4-6 digit pin code, all weather keypad and housing, keypad or computer programming, 32 user groups, multi-year scheduling, temporary users, multiple zones, real time clock, auto daylight savings adjustment and more.
           2. E77P shall operate on 4 AA Batteries and shall have REX and DPS inputs with an AUX Relay Output (SPDT, 1A @ 30VDC)
           3. HID compatible Proximity card reader and/or Proximity FOB reader
           4. ¾” (19mm) throw deadlocking Stainless Steel Pullman Latch bolt
           5. UL & ULC Listed panic and fire exit hardware. ANSI/BHMA A156.3-2001 Grade 1 Compliant. CA Title 19 Compliant. Meets/Exceeds ADA requirements. UBC 97, Standard 7.2.
           6. Levers - Galaxy and Eclipse return to within 1/2 inch (13mm) of the door face.

\*\* NOTE TO SPECIFIER \*\* Lever Handles with/without cylinders. Delete lever not required.

* + - 1. Specify Keypad Finish

1. Q – 626 Dull Chrome (Standard)
2. B - Black
   * + 1. Specify Electrically Operated Escutcheon Trim Style. 626 Dull Chrome finish (Q)
3. EKM – Eclipse (Less Cylinder)
4. GKM – Galaxy (Less Cylinder)
   * + 1. Exit Bar Part Number – 61 (Standard S6100 Rim Exit Bar)
       2. Specify Panic or Fire Rated Exit bar
5. P – Panic Exit device with mechanical dogging
6. F – Fire Rated Exit bar (Mechanical dogging not allowed)
   * + 1. Exit bar finish shall be – (U) 630 Stainless Steel
       2. Specify Exit Bar length – 36” or 42” or 48”
       3. Optional Mortise Cylinder for Trim
7. CYL-6KDQ – 6 pin, 1-1/8” Mortise Cylinder, Keyed different, 626 Dull Chrome
8. CYL-6KAQ – 6 pin, 1-1/8” Mortise Cylinder, Keyed alike, 626 Dull Chrome
   * + 1. Optional - Card: HID1326-100 ProxCard II (100 cards) as manufactured by SDC Security Door Controls.
       2. Optional - Card: HID1326-25 ProxCard II (25 cards) as manufactured by SDC Security Door Controls.
       3. Optional - Key Fob: HID1346-10 ProxKey II (10 key fobs) as manufactured by SDC Security Door Controls.
       4. Optional - Key Fob: HID1346-100 ProxKey II (100 key fobs) as manufactured by SDC Security Door Controls.